

**REPUBLIC OF CROATIA**

**DUBROVNIK-NERETVA COUNTY**

Administrative Department for

Physical Planning, Construction and

Environmental Protection

Pred Dvorom 16, Dubrovnik

CLASS: 351-02/11-01/89

REG. NO.: 2117/1-23/1-12-11-02

Dubrovnik, 21 September 2011

Pursuant to Article 38, paragraph 2 of the Nature Protection Act (Official Gazette 70/05, 139/08, 57/11), in the procedure of issuing a location permit for constructing a siphon under the Mala Neretva watercourse with a pipeline from PS Prag to the drainage channel in Glogačko Lake (Class: UP/I-350-05/11-01/126), employer Hrvatske vode, Regional Office Split, the Administrative Department for Physical Planning, Construction and Environmental Protection of Dubrovnik-Neretva County hereby defines the following

**SPECIAL NATURE PROTECTION REQUIREMENTS**

1. During construction of the siphon pipeline under the Mala Neretva river, care shall be taken that underwater works are carried out in the shortest possible period, avoiding the spawning period of the fish depositing their eggs into the silt on the river bottom.
2. During construction of the pipeline on the right bank of the Mala Neretva from station 0+060.00 to the connection with the drainage channel in Glogačko Lake, care shall be taken about providing maximum protection to the valuable vegetation along the Mala Neretva and to valuable agricultural plots, by laying the pipeline into the route of the existing field paths, cut-offs or along the edge of agricultural plots. When excavating ditches into which the pipeline will be laid, the top soil or surface soil layer shall be disposed separately and used for backfilling the ditches, when it shall again be placed on the surface.
3. The movement of heavy machinery shall be limited, i.e. the zone in which machinery moves shall be minimised, using to the maximum possible extent the existing network of roads, which shall be restored after the completion of construction works.
4. The excavated material shall be used for backfilling the ditches. Excess excavation material and construction waste shall be regularly removed from the construction site and, depending on the waste type, handed over to the authorised waste collecting or recycling company.
5. Upon the completion of works, the structures and machinery used for construction shall be removed and the area in which the works were done shall be restored and improved.

Acting Head

Nikolina Šišić, LL.B.

To be delivered to:

1. Dubrovnik-Neretva County, Administrative Department for Physical Planning, Construction and Environmental Protection, Metković Office, Ulica kralja Zvonimira 22, 2035 Metković
2. Records, here
3. Files, here

Cc:

1. Ministry of Culture, Directorate for Nature Protection

Runjaninova 2, 10000 Zagreb